DusVERA

**ELECTRONIC SURFACE-MOUNTED CODE LOCK WITH BATTERY POWER FOR INSERT LOCKS**

**FEATURES**

* Electronic surface-mounted code lock.
* To be combined with an insert lock.
* Battery operated.
* Vandal-proof battery compartment.
* Mounting on a flat surface, on the gate profile or gate cladding
* Different handles available.
* Choice of single-sided code keyboard with cover plate or double-sided code keyboard
* Up to 100 different input and output codes possible.
* Free exit possible via handle
* Permanently open code possible.
* Warning indication “battery almost empty”.
* Available in silver and RAL 9005.
* Designed and produced in Europe or the United States.

**PERFORMANCE**

* Developed for outdoor use.
* IP66
* Tested for at least 500,000 movements.
* Maintenance-free
* 2 years factory warranty.
* Battery pack life: 150,000 open/close cycles.

**INSTALLATION**

* Mounting via 2 bolts.
* Programming via Master PIN code.
* Installation video available.

**MATERIAL**

* Aluminium housing.
  + Black version: fine textured powder coating in accordance with the Qualicoat standard
  + Silver version: anodization
* Rust resistance of 1000h salt spray test in accordance with ISO9227.
* Push buttons:
  + Black version: black anodized aluminium.
  + Silver version: stainless steel.