HELIOS
**ARCHITECTURAL OUTDOOR LIGHTING**

**FEATURES**

* Wall Lighting
* Aluminium housing
* It is suitable for installation on all surfaces.
* Standard colours: black, silver, anthracite and bronze
* Variants can be painted to suit preferences.
* Connection:
	+ 230V AC
	+ 12-24V DC
* Colour temperature: 2700K
* Widths: from 55 mm to 85 mm
* Heights: from 64 mm to 100 mm
* Designed and manufactured in Europe or the United States

**PERFORMANCE**

* Developed for outdoor use.
* IP65 rating.
* Energy-efficient LED technology
* Lifespan: 50,000 burning hours
* Luminous flux:
	+ 300 lumens (230V AC)
	+ 270 lumens (12-24V DC)
* Energy consumption:
	+ 4.6W (230V AC)
	+ 3W (12-24V DC)
* 2 years warranty

**INSTALLATION**

* Uniform hole pattern
* QUICK-FIX mounting
* Installation with standard tools and Allen key
* WAGO connectors
* Both parallel and serial connections are possible.

**MATERIAL**

* Aluminium hood
* Powder coating applied in compliance with the Qualicoat standard.